IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "C:\\Dropbox\\Acad\\_Renovum\\_Hicon\\_Totaal hekken eenvoudig weergegeven.ifc"
Time stamp: "2024-04-10T11:36:34"
Author: "Undefined"
Organization: "Undefined"
Preprocessor: "BricsCAD BIM 23.1.08"
Originating system: "BricsCAD BIM 23.1.08"
Authorization: "Undefined"
Application: "BricsCAD BIM" version "V23" identifier "Bcad" by Organization "Bricsys"

People and organizations
  Person "Bricsys" of Organization "Bricsys"
  Owner history of Person "Bricsys" of Organization "Bricsys" | application "BricsCAD BIM" version "V23" identifier "Bcad" by Organization "Bricsys" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: RADIAN
  TIMEUNIT: SECOND
  MASSUNIT: GRAM

Spatial structure
IFCPROJECT "_Totaal hekken eenvoudig weergegeven"
  IFCSITE "Site" | latitude 52° 22′ 22.799999″ | longitude 4° 53′ 41.279999″ | elevation above sea level 0.
    contains 117 elements
      3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "info"
      4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Eindbaluster_80x8 voor Lamelhek"
      4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Hekdeel SPR70X21+SPR70X21 lg2085 h950 0° 45°"
      2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Hekdeel SPR70X21+SPR70X21 lg2130 h950 45° 45°"
      4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Hekdeel SPR70X21+SPR70X21 lg2085 h950 45° 0°"
      4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "kb-Hoekbaluster_90°_80x8 voor Lamelhek"
      4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Eindbaluster_1200_80x8 voor Lamelhek"
      4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "kb-Hoekbaluster_1200_90°_80x8 voor Lamelhek"
      3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "handlijst hr70x35 rondom 2200"
      6 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Hicon balkon lg2000"
      4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Eindbaluster_80x8 voor gr60x35"
      4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "kb-Hoekbaluster_90°_80x8 voor gr60x35"
      4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Hekdeel GR60X35O+GR60X35B lg2093 h950 0° 45°"
      2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Hekdeel GR60X35O+GR60X35B lg2141 h950 45° 45°"
      4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Hekdeel GR60X35O+GR60X35B lg2093 h950 45° 0°"
      4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Eindbaluster_1200_80x8 voor gr60x35"
      4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "kb-Hoekbaluster_1200_90°_80x8 voor gr60x35"
      4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Eindbaluster_80x8 voor GR45x35"
      4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "kb-Hoekbaluster_90°_80x8 voor GR45x35"
      4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Hekdeel GR45X35+GR45X35 lg2220 h960 0° 45°"
      2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Hekdeel GR45X35+GR45X35 lg2258 h960 45° 45°"
      4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Hekdeel GR45X35+GR45X35 lg2220 h960 45° 0°"
      4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Eindbaluster_1200_80x8 voor GR45x35"
      4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "kb-Hoekbaluster_1200_90°_80x8 voor GR45x35"
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tussenbaluster_1200_80x8"
      2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Hekdeel GR45X35+GR45X35 lg1327 h960 45° 0°"
      2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Hekdeel GR45X35+GR45X35 lg1327 h960 0° 45°"
      3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "handlijst hr70x35 rondom 2600"
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tussenbaluster_1200_80x8 voor GR45x35"
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tussenbaluster_1200_80x8 voor gr60x35"
      2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Hekdeel lg1255 GR60X35O+GR60X35B h950 45° 0°"
      2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Hekdeel lg1255 GR60X35O+GR60X35B h950 0° 45°"
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tussenbaluster_1000_80x8 voor gr60x35"
      2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Hekdeel lg1255 SPR70X21+SPR70X21 h950 0° 45°"
      2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Hekdeel lg1255 SPR70X21+SPR70X21 h950 45° 0°"
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tussenbaluster_1200_80x8 voor Lamelhek"
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Tussenbaluster_1000_80x8 voor Lamelhek"
      6 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Hicon balkon lg2400"
    IFCBUILDING "Site" | reference height above sea level 0. | terrain above sea level 0.

Types
  IFCBUILDINGELEMENTPROXYTYPE "info" | 3 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Eindbaluster_80x8 voor Lamelhek" | 4 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Hekdeel SPR70X21+SPR70X21 lg2085 h950 0° 45°" | 4 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Hekdeel SPR70X21+SPR70X21 lg2130 h950 45° 45°" | 2 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Hekdeel SPR70X21+SPR70X21 lg2085 h950 45° 0°" | 4 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "kb-Hoekbaluster_90°_80x8 voor Lamelhek" | 4 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Eindbaluster_1200_80x8 voor Lamelhek" | 4 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "kb-Hoekbaluster_1200_90°_80x8 voor Lamelhek" | 4 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "handlijst hr70x35 rondom 2200" | 3 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Hicon balkon lg2000" | 6 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Eindbaluster_80x8 voor gr60x35" | 4 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "kb-Hoekbaluster_90°_80x8 voor gr60x35" | 4 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Hekdeel GR60X35O+GR60X35B lg2093 h950 0° 45°" | 4 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Hekdeel GR60X35O+GR60X35B lg2141 h950 45° 45°" | 2 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Hekdeel GR60X35O+GR60X35B lg2093 h950 45° 0°" | 4 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Eindbaluster_1200_80x8 voor gr60x35" | 4 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "kb-Hoekbaluster_1200_90°_80x8 voor gr60x35" | 4 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Eindbaluster_80x8 voor GR45x35" | 4 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "kb-Hoekbaluster_90°_80x8 voor GR45x35" | 4 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Hekdeel GR45X35+GR45X35 lg2220 h960 0° 45°" | 4 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Hekdeel GR45X35+GR45X35 lg2258 h960 45° 45°" | 2 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Hekdeel GR45X35+GR45X35 lg2220 h960 45° 0°" | 4 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Eindbaluster_1200_80x8 voor GR45x35" | 4 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "kb-Hoekbaluster_1200_90°_80x8 voor GR45x35" | 4 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Tussenbaluster_1200_80x8" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Hekdeel GR45X35+GR45X35 lg1327 h960 45° 0°" | 2 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Hekdeel GR45X35+GR45X35 lg1327 h960 0° 45°" | 2 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "handlijst hr70x35 rondom 2600" | 3 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Tussenbaluster_1200_80x8 voor GR45x35" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Tussenbaluster_1200_80x8 voor gr60x35" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Hekdeel lg1255 GR60X35O+GR60X35B h950 45° 0°" | 2 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Hekdeel lg1255 GR60X35O+GR60X35B h950 0° 45°" | 2 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Tussenbaluster_1000_80x8 voor gr60x35" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Hekdeel lg1255 SPR70X21+SPR70X21 h950 0° 45°" | 2 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Hekdeel lg1255 SPR70X21+SPR70X21 h950 45° 0°" | 2 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Tussenbaluster_1200_80x8 voor Lamelhek" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Tussenbaluster_1000_80x8 voor Lamelhek" | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "Hicon balkon lg2400" | 6 occurrences